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Congratulations on your purchase of our Acacia Canopy Juniper model. This unit is a combination of excellent manufacturing and design. It is comprised of a rigid frame and a durable cover. For easy assembly, we have marked all the parts with codes. With proper installation, use and maintenance, your unit will provide many years of good and suitable service.

READ ALL THE INSTRUCTIONS BEFORE ASSEMBLY！
1. The proper erection and installation of this building requires a high level of care and safety. We recommend the safety regulations be complied with during the installation. It includes but is not limited to:
· Safety hats, protective eyewear, protective clothing and protective gloves
· Safety harnesses for all elevated workers
· Proper ladder, cage, and safety operation
2. Site selection: Choose a solid level location for your building. Do not install the building where the ground could not keep the building steady. Do not install the building where the ground could not bear the weight of the building. Do not install the building in soft grass ground or wetland.
3. Be cautious with the surroundings. Keep work area clean. Do not set up it near snow drifts, in slippery places, or in wet location. The cover of the building will protect against normal falling leaves and light debris, however, large, fast or sharp falling items etc. may cause a puncture or tear in the cover material. So, keep the building away from such harmful things. Be careful with power and heat sources. Don’t keep heat sources, flammable and explosive hazardous goods near the tarpaulin. Don’t expose to open flame.
4. Chose a windless day to install the building. It is very difficult to attach the cover in heavy wind. Do not install your building where there usually has strong wind. Please remove or roll up the tarpaulin of the building during strongly windy days. If worrying about suffering strong wind, please use cement to fix base flange and hammer the pegs into the cement when it not solidified.
5. If the instructions in the manual are not followed, we are not responsible for any damage or accident.
   Don’t make alteration of the frame. 

ITEMS NEEDED FOR INSTALLATION
1. Cherry Picker 
2. 19mm and 17mm Spanner and socket set
3. Welder
4. Duct Tape



ASSEMBLY PROCEDURE
1. Prepare the location and place all unit boxes near sight. Perform an inventory check before beginning, to be certain all components are available for installation.
2. Secure base plates flanges to base surface.
3. Assemble all groups of arches.
4. Begin frame assembly with front end arch, first interior arch, purlins, etc.
5. Add to assemble other groups of arches.
6. Install main cover over frame. 
7. Install end covers over end panels.
Read all the detailed instructions and notices in the following assembly instructions!

MAINTENANCE AND CARE
1. If some parts or the cover were accidently damaged during the use, contact the local supplier for advice on the repairing method.
2.  When attaching the cover, choose a windless day. Begin with making certain all the bolts of the frame and the tensioning equipment are well fixed. 
3. To extend the life of the cover, put small duct tape or foam rubber (provide by yourself) on the frame that comes to in contact with cover. The tape and foam rubber acts as a cushion to avoid rubbing damage to the cover over years.
4. Periodically the canopy should be completely inspected and maintained internally and externally to make sure the canopy remains properly installed and secured. Including: check all bolts and hardware connectors to be certain they are in place and tightened, the base plates are still fixed firmly, check and adjust the ropes if in need, clean the cover with suitable washing. Allowing dirt and debris to sit on cover over an extended time will damage cover irreparably.

Thanks again for choosing this quality product. The following is the detailed assembly instructions for you starting the assembly.





	



	PARTS LIST

	PART #
	DESCRIPTION
	QUANTITY

	L1
	Base Plate
	9

	R1
	Base Plate
	9

	1
	3 Way Joint (Ends)
	2

	2
	4 Way Joints
	7

	3
	Top Portal
	18

	4
	Side Portal
	18

	5
	Ridge Purlin
	8

	6
	Connection Purlin
	32

	7
	Tensioning Tube
	2 sets

	8
	Choke Rope Bracket
	4

	9
	Roof Cover
	1

	10
	End Plugs for tensioning tube
	4

	11
	Lacing Rope for cover
	

	12
	Bolt - M8 x 60
	110

	13
	Bolt - M8 x 70
	36

	14
	Butterfly Bolt
	16

	15
	Ratchets and Straps
	18











CONTAINER SHELTER ASSEMBLED FRAME
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Assemble all individual frames on the ground

 
STEP 1 - CONTAINER LAYOUT & POSITIONING
1. Both containers should be of equal height and on firm, level ground. Position containers 5.8m apart.

2. Note: If containers are not fixed to concrete piers for anchorage, they should be
ballasted. Suggest minimum of 500kg per metre for length of each container.

Standard 40' container layout diagram
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3. Do not proceed to further assembly until proper fixing or weighting of the containers 
has happened.









STEP 2 - BASE PLATE LAYOUT 12.0m (40')
Note the position of base plate (Parts #R1) on diagram.
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STEP 3 - BASE PLATE FIXING
1. Position the base plates (Parts #L1 & #R1) to the container tops. Note the positions of 
base plates on layout diagrams Step 2.
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2. Weld the base plate to the container tops securely.

3. Weld the 4 Choke Rope Brackets (Part #8) to the inside edges of the containers, approximately 300mm directly below each of the corner base plates.




STEP 4 - PORTAL ASSEMBLY
1. Assemble ALL individual portals on the ground first.
2. On both end portals, use 2 x Part #4 (side portals), 2 x Part #3 (top portal) & 1 x Part #1 (3 way joints).
3. Internal portals use 2 x Part #4 (side portals), 2 x Part #3 (top portal) & 1 x Part #2 (4 way joints).
4. Bolt together using bolts - Part #12 (M8 x 60).
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STEP 5 - FRAME ASSEMBLY CONT'
1. Lift fully assembled end portal (3 way joint) onto the secured corner base plates at both ends.
2. Drop the portal legs onto the spigots of the base plate on one side, and gently ease portal in and drop down onto spigot on opposite side (portals go in under tension) and secure using bolt Part #12. 
3. Repeat this process with the remaining internal portals (portal with 4 way joints).
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STEP 6 - FRAME ASSEMBLY CONT'
1. Connect all portals at centre top with the ridge purlin (Part #5) and butterfly bolts (Part #14).
2. Continue connecting portals with remaining connection purlins (Part #6), 'Connection Purlins' using Bolt (Part #13).
3. Purlins overlap each other at flattened ends and bolt passes through top of portal down through each purlin, to be tightened with nut from underside.
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STEP 7 - PREPARE MAIN COVER
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1. Unfold cover carefully and locate the two end pouches which contain the choke ropes, 
already threaded through. There will also be a row of eyelets on the underside of each end close to the choke rope pouch.
2. The underside of the cover also has a sleeve running along each side which will hold 
the tensioning tubes.
3. Position cover on one side of the shelter with the eyelets and sleeve on underside ready 
to slide over frame.
4. Insert tensioning tubes (Part #7) into the sleeve on the lead side, install end plugs (Part 
#10) on to 2 ends of tube sets. Tie ropes onto the tensioning tubes through the small slits which were cut on the sleeve. Throw ropes over to opposite side of shelter.
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Installing end plugs                       Insert tensioning tubes
STEP 8 - COVER INSTALLATION
CAUTION: DO THIS ONLY WHEN THERE IS LITTLE OR NO WIND
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Note: Ensure the cover is the right way around and have an even amount of cover overhanging at both ends of the frame. Sleeves are on the underside and are on the sides of the cover only. The ends of the cover have the choke ropes already threaded through as well as the eyelets on underside.

1. Insert the tensioning tubes (Parts #7) into the sleeves on both sides of the cover, install 
end plugs (Part #10) on to the 4 ends of the tube sets. Tie rope to the tensioning tube at equidistant points along the side to be pulled over.
2. Position one man per rope, standing on the ground on the other side of the container.
3. Collectively ease the cover over the top of the frame from one side to the other, 
checking that the cover is not catching on any purlins from underside. Work steadily & evenly without excessive force.


4. Once the cover is square on the frame, ensure even overhang at both ends and even 
height on both sides. Immediately secure the four corners using the choke ropes to the choke rope brackets.
5. Double check that cover continues to be square on the frame.
6. Fix & re-tension the choke ropes securely at each end to the bracket.









STEP 9 - COVER TENSIONING
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Installing ratchets and straps
1. Lace the underside of the main over to end portals of the shelter using the eyelets on 
the cover and the lacing rope (Part #11). Start lacing from the centre top and work evenly down each side to the base plates. Only secure the ends of the lacing rope to the frame. Do not tie off to the cover.
2. Cut small incisions into the tensioning tube sleeves directly above each ratchet on each 
base plate. The incision should be wide enough for the ratchet strap to slide through. CAUTION-DO NOT CUT THROUGH THE MAIN COVER, ONLY THE SLEEVE CONTAINING THE TENSIONING TUBE.
3. Thread the ratchet webbing strap over the tensioning tube at each ratchet location and 
feed the end through the steel loop on the base plate. Thread the ends of the strap into the tie down ratchet. Tension only loosely at this stage until all ratchets have been loaded.
4. Once all ratchets are loaded, progressively tension each ratchet properly starting at the center ratchet and working evenly out to the ends on each container. This will ensure even tension is spread over the cover and that there are no wrinkles in the cover.

5. Check again the lacing rope, retension if necessary, and check that the choke ropes are all tight and that all knots are tied securely.
6. After a day or two the cover may settle on the frame further, and you will be required to recheck the tensioning of all the ratchets, the lacing and the choke ropes. It is important to maintain good tension of the cover on the frame at all times. You should not be able to get your hand between the cover and the portals.
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